			AC97 Mixer
			Version 1.5

AC97 Mixer allow direct access to AC97 compatible audio codec present on the
PCI sound card. It can display codec specific information, including vendor,
model and DAC/ADC resolution. Also it can be used to change codec specific
controls, not available in standard Windows mixer driver.

PCI audio controllers supported:
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
- Yamaha YMF724, YMF740, YMF744, YMF754
- Aureal AU8830 (Vortex 2, MX300)
- VIA integrated VT82C686A
- Creative EMU10K1 (not tested)
- Intel 8x0, MX440 (not tested)
- Ensoniq ES1371/ES1373 (SB64)
- ESS Maestro 1/2/2E (not tested)
- Cirrus Logic CS461x (not tested)

Installation:
~~~~~~~~~~~~~
- Unzip all files into the destination directory
- Run 'wdreg install'

Known issues:
~~~~~~~~~~~~~
- 

Revision history:
~~~~~~~~~~~~~~~~~
Version 1.5
- added support for ESS Maestro 1/2/2E
- added support for Cirrus Logic CS461x
- added File | Save... menu command

Version 1.4
- added rear (surround) volume fader for 4 channel codecs
- yet another bugfix in the Intel 8x0 support

Version 1.3
- added support for Ensoniq ES1371/ES1373
- bugfix in the Intel 8x0 support
- some faders reversed
- added reset mixer menu command

Version 1.2
- added support for Creative EMU10K1
- added support for Intel 8x0, MX440
- bugfixes

Version 1.1
- added support for Aureal AU8830
- added support for VIA VT82C686A
- bugfixes

Version 1.0
- initial release


This program still in the beta stage - so be patient -:)
Feel free to send your feedback to usyst@gu.net

Copyright (C) by Alex Mina, 2000